{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["1-采购公告摘录表","2-报价清单"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1-采购公告摘录表","index":0,"n_rows":25,"n_cols":3,"rows_kept":25,"merged":[[0,0,0,2],[2,0,5,0],[8,1,8,2],[13,0,14,0],[13,1,14,1],[16,1,16,2]],"flags":["formulas_cached_only"]}
["采购方案摘要表"]
["序号","条款名称","具体内容"]
["项目基本内容","标段名称","华能天镇武家山场站9台风机顶端塔筒垂直电缆防护圈改造工程采购"]
[null,"项目概况","    华能天镇武家山场站位于山西省大同市天镇县，于2012年6月投产运行，风电总装机99MW，安装浙江运达风电股份有限公司WD1500-82机组66台。风机变频器放置在塔下，发电机主电缆和控制电缆由机舱穿至塔底，机组顶端的电缆支架和抱箍固定在梯子上，由于爬梯材质为铝合金，强度不足，导致电缆支架和抱箍晃动严重，长时间运行后可能发生梯子变形或电缆磨损。为保证运行安全，场站计划对电缆防护圈进行改造。将支架固定点移至爬梯与塔筒固定耳处，并重新制作电缆支架和抱箍将9台风机损坏的支架和抱箍进行替换。"]
[null,"采购单位","华能天镇风力发电有限公司"]
[null,"采购范围","工程内容主要包括将9台风机顶端塔筒垂直电缆防护圈进行改造。将固定点移至爬梯与塔筒固定耳处，并重新制作电缆支架和抱箍将9台风机损坏的支架和抱箍进行替换。"]
[1,"采购方式","本项目资金来源为 企业自筹 ，该项目已具备采购条件，现对采购项目进行公开询价。"]
[2,"评审办法","经评审的最低价法"]
[3,"专项条件"]
[3.1,"资质要求","无"]
[3.2,"业绩要求","至少具有5台风机改造业绩（附合同首页、内容页、签字盖章页等关键页）"]
[3.3,"是否接受联合体投标","本次采购不接受联合体投标。"]
[3.4,"是否接受代理商投标","本次采购不接受代理商投标。"]
[3.5,"其他要求","禁止失信被执行人、行贿受贿行为人、法律所禁止的存在关联关系供应商参与采购活动。"]
[null,null,"其他要求：无。"]
[3.6,"踏勘现场","自行踏勘"]
[4,"合同条款"]
[4.1,"付款要求","1.本工程不支付预付款。\n2.付款方式：银行转账\n3.付款条件：\n3.1经甲方验收合格后3个月内改造后的防护圈无变形、电缆无磨损支付100%合同款；\n3.2付款时需附资料见合同付款条款。"]
[4.2,"质保期","无"]
[4.3,"验收标准","详见技术文件第四条验收标准"]
[4.4,"工期要求","合同签订之日起30个自然日内完工。"]
[4.5,"施工、服务\n或交货地址","山西省大同市天镇县武家山风电场"]
[4.6,"合同违约及考核条款","执行商务通用条款。"]
[4.7,"合同条款特殊要求","无"]
[4.8,"备注","投标人应提前做好应对措施，保证在采购人要求的时间内按时完工，不得以现场考虑不周、情况了解不细或疫情等因素为由影响工期，由此造成的一切后果由投标人自行承担。"]

{"sheet":"2-报价清单","index":1,"n_rows":4,"n_cols":7,"rows_kept":4,"merged":[[0,0,0,6],[3,1,3,4],[5,0,5,6]],"flags":["formulas_cached_only"]}
["工程量清单"]
["序号","名称","单位","数量","单价","合计","备注"]
[1,"9台风机顶端塔筒垂直电缆防护圈更换改造工程","套",11,null,null,"1.08#、15#、16#、17#、29#、30#、32#七台风机，每台需要安装1个电缆防护圈；45#、47#两台风机，每台需要安装2个电缆防护圈。2.本次报价包含但不限于支架及抱箍等材料费。"]
["合计","大写：                  ",{"$nulls":4},"请注明发票类型及税率"]